RacePak NOS Gauge Instructions



To Set Backlight Color (cool white / warm white):

1. Start with power off.
2. Press and hold the pushbutton.
3. While pressing the pushbutton, apply power to the gauge (starting vehicle not necessary).
4. Release pushbutton once power is applied.
5. The pointer will indicate 900 PSI. 
6. Tap the push button to move the pointer to 0 PSI.
7. With the pointer indicating 0 PSI, press and hold the pushbutton until the pointer moves to 450 PSI or 1350 PSI.
8. 450 PSI represents the “cool white” lighting option, and 1350 PSI represents the “warm white” lighting option.  Tap the pushbutton to move the pointer between 450 PSI and 1350 PSI.
9. When the pointer indicates the desired lighting option, press and hold the pushbutton until the pointer returns to 0 PSI.  Turn off power to save the changes.




To Set Warning Light Trigger Point:

1. Start with power off.
2. Press and hold the pushbutton.
3. While pressing the pushbutton, apply power to the gauge (starting vehicle not necessary).
4. Release pushbutton once power is applied.
5. The pointer will indicate 900 PSI. 
6. Tap the pushbutton twice to move the pointer to 0 PSI and back to 900 PSI again.
7. Press and hold the pushbutton (with the pointer at 900 PSI) until the pointer moves to indicate the warning light trigger point.
8. Press and hold the pushbutton to change the trigger pressure shown.  The first time the pushbutton is pressed and held, the pressure shown will increase.  The second time the pushbutton is pressed and held, the pressure shown will decrease.  The pressure shown will alternate between increasing and decreasing each time the pushbutton is pressed.
9. The warning light will come on when the pressure is above the trigger pressure.
10. Once the desired trigger point is shown, wait 10 seconds without pushing the pushbutton in order to save the setting.  The pointer will return to 0 PSI.  Turn off power to save the changes.


Important:  Turn power OFF to the gauge after making changes in order to save those changes
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Optional Data Logger Output:

0.5V to 4.5V Linear Scale Output

0.5V = 0 PSI

4.5V = 1800 PSI

Remote Warning Light Ground  [YELLOW / WHITE]
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Optional Remote Warning Lt. Trigger:

Provides a 

ground

 for a remote warning light

(30mA max) at user specified temperature.

Run 12V to light separately.
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